Fibr e Channel Upgrade fr om FC version 3.0 to FC version 4.3.

All the Fibre Channel equipment available at CERN on the 24^{th} of April 1995 has been upgraded to 4.3 Fibre Channel Standard. Below is an overview of the different types of interfaces that are constituting our heterogeneous Fibre Channel Architecture (in parenthesis are the workstations in which these interfaces are located):

2 ANCOR-MCA FC interfaces (IBM RS/6000-250, IBM RS/6000-590), 2 IBM-MCA FC interfaces (IBM RS/6000-41T), 3 ANCOR-EISA FC interfaces (HP/9000-735).

The picture hereinafter displays the full Fibre Channel Architecture:

ANCOR FIBRE CHANNEL FABRIC

RS/6000-590

RS/6000-250

HP/9000-735

(rsibm3, fcsibm3)

(rsibm1, fcsibm1)

(hpfcs1, hpfcsf1)

HP/9000-735 (hpfcs3, hpfcsf3)

HP/9000-735 (hpfcs2, hpfcsf2)

RS/6000-41T (rsfcs1,fcsfcs1)

RS/6000-41T (rseff1, fcseff1)

1 2 3 4 5 6 7 8

9 10 11 12 13 14 15 16